| GQLLC GMC-300 0.1 GQ Electronics Geiger-Counter Model 300

- Main Page
- Namespaces
- Classes
- Files

- Class List
- Class Index
- Class Members

- All
- Functions
- Variables
- Enumerator

- a
- b
- c
- d
- g
- i
- m
- n
- p
- r
- s
- z

### - a -

- alarmCPMValueHiByte : GQLLC::GQGMC::cfg_data_t
- alarmCPMValueLoByte : GQLLC::GQGMC::cfg_data_t
- alarmOnOff : GQLLC::GQGMC::cfg_data_t
- alarmType : GQLLC::GQGMC::cfg_data_t
- alarmValueuSvUcByte0 : GQLLC::GQGMC::cfg_data_t
- alarmValueuSvUcByte1 : GQLLC::GQGMC::cfg_data_t
- alarmValueuSvUcByte2 : GQLLC::GQGMC::cfg_data_t
- alarmValueuSvUcByte3 : GQLLC::GQGMC::cfg_data_t

### - b -

- backlightTimeoutSeconds : GQLLC::GQGMC::cfg_data_t
- bScroll : Plotter

### - c -

- c : HexCharStruct
- calibrationCPMHiByte_0 : GQLLC::GQGMC::cfg_data_t
- calibrationCPMHiByte_1 : GQLLC::GQGMC::cfg_data_t
- calibrationCPMHiByte_2 : GQLLC::GQGMC::cfg_data_t
- calibrationCPMLoByte_0 : GQLLC::GQGMC::cfg_data_t
- calibrationCPMLoByte_1 : GQLLC::GQGMC::cfg_data_t
- calibrationCPMLoByte_2 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte0_0 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte0_1 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte0_2 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte1_0 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte1_1 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte1_2 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte2_0 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte2_1 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte2_2 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte3_0 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte3_1 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte3_2 : GQLLC::GQGMC::cfg_data_t
- curveMap : Plotter
- curZoom : Plotter

### - d -

- dataReadAddress0 : GQLLC::GQGMC::cfg_data_t
- dataReadAddress1 : GQLLC::GQGMC::cfg_data_t
- dataReadAddress2 : GQLLC::GQGMC::cfg_data_t
- dataSaveAddress0 : GQLLC::GQGMC::cfg_data_t
- dataSaveAddress1 : GQLLC::GQGMC::cfg_data_t
- dataSaveAddress2 : GQLLC::GQGMC::cfg_data_t

### - g -

- graphicModeOnOff : GQLLC::GQGMC::cfg_data_t

### - i -

- idleDisplayMode : GQLLC::GQGMC::cfg_data_t
- idleTitleDisplayMode : GQLLC::GQGMC::cfg_data_t

### - m -

- maxBytes : GQLLC::GQGMC::cfg_data_t
- maxCPMHiByte : GQLLC::GQGMC::cfg_data_t
- maxCPMLoByte : GQLLC::GQGMC::cfg_data_t
- maxX : PlotSettings
- maxY : PlotSettings
- mBig_endian : GQLLC::GQGMC
- mCFG_Data : GQLLC::GQGMC
- mCPS_is_on : GQLLC::GQGMC
- mError_code : GQLLC::GQGMC
- mFirmware_revision : GQLLC::GQGMC
- mHistory_data : GQLLC::GQGMC
- minX : PlotSettings
- minY : PlotSettings
- mRead_status : GQLLC::GQGMC
- mUSB_device : GQLLC::GQGMC
- mUSB_serial : GQLLC::GQGMC
- myTimerID : Plotter

### - n -

- nCounterDelayHiByte : GQLLC::GQGMC::cfg_data_t
- nCounterDelayLoByte : GQLLC::GQGMC::cfg_data_t
- nPowerSavingMode : GQLLC::GQGMC::cfg_data_t
- nSensitivityAutoModeThreshold : GQLLC::GQGMC::cfg_data_t
- nSensitivityMode : GQLLC::GQGMC::cfg_data_t
- numXTicks : PlotSettings
- numYTicks : PlotSettings
- nVoltageOffset : GQLLC::GQGMC::cfg_data_t

### - p -

- pixmap : Plotter
- powerOnOff : GQLLC::GQGMC::cfg_data_t

### - r -

- rubberBandIsShown : Plotter
- rubberBandRect : Plotter

### - s -

- sampleCnt : Plotter
- saveDataType : GQLLC::GQGMC::cfg_data_t
- saveDateTimeStampByte0 : GQLLC::GQGMC::cfg_data_t
- saveDateTimeStampByte1 : GQLLC::GQGMC::cfg_data_t
- saveDateTimeStampByte2 : GQLLC::GQGMC::cfg_data_t
- saveDateTimeStampByte3 : GQLLC::GQGMC::cfg_data_t
- saveDateTimeStampByte4 : GQLLC::GQGMC::cfg_data_t
- saveDateTimeStampByte5 : GQLLC::GQGMC::cfg_data_t
- spare : GQLLC::GQGMC::cfg_data_t
- speakerOnOff : GQLLC::GQGMC::cfg_data_t
- swivelDisplay : GQLLC::GQGMC::cfg_data_t

### - z -

- zoomByte0 : GQLLC::GQGMC::cfg_data_t
- zoomByte1 : GQLLC::GQGMC::cfg_data_t
- zoomByte2 : GQLLC::GQGMC::cfg_data_t
- zoomByte3 : GQLLC::GQGMC::cfg_data_t
- zoomInButton : Plotter
- zoomOutButton : Plotter
- zoomStack : Plotter

All Classes Namespaces Files Functions Variables Enumerations Enumerator