| GQLLC GMC-300 0.1 GQ Electronics Geiger-Counter Model 300

- Main Page
- Namespaces
- Classes
- Files

- Class List
- Class Index
- Class Members

- All
- Functions
- Variables
- Enumerator

- a
- b
- c
- d
- e
- g
- h
- i
- k
- l
- m
- n
- o
- p
- r
- s
- t
- u
- w
- z
- ~

Here is a list of all class members with links to the classes they belong to:

### - a -

- adjust() : PlotSettings
- adjustAxis() : PlotSettings
- alarmCPMValueHiByte : GQLLC::GQGMC::cfg_data_t
- alarmCPMValueLoByte : GQLLC::GQGMC::cfg_data_t
- alarmOnOff : GQLLC::GQGMC::cfg_data_t
- alarmType : GQLLC::GQGMC::cfg_data_t
- alarmValueuSvUcByte0 : GQLLC::GQGMC::cfg_data_t
- alarmValueuSvUcByte1 : GQLLC::GQGMC::cfg_data_t
- alarmValueuSvUcByte2 : GQLLC::GQGMC::cfg_data_t
- alarmValueuSvUcByte3 : GQLLC::GQGMC::cfg_data_t

### - b -

- backlightTimeoutSeconds : GQLLC::GQGMC::cfg_data_t
- bScroll : Plotter

### - c -

- c : HexCharStruct
- calibrationCPMHiByte_0 : GQLLC::GQGMC::cfg_data_t
- calibrationCPMHiByte_1 : GQLLC::GQGMC::cfg_data_t
- calibrationCPMHiByte_2 : GQLLC::GQGMC::cfg_data_t
- calibrationCPMLoByte_0 : GQLLC::GQGMC::cfg_data_t
- calibrationCPMLoByte_1 : GQLLC::GQGMC::cfg_data_t
- calibrationCPMLoByte_2 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte0_0 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte0_1 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte0_2 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte1_0 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte1_1 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte1_2 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte2_0 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte2_1 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte2_2 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte3_0 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte3_1 : GQLLC::GQGMC::cfg_data_t
- calibrationSvUcByte3_2 : GQLLC::GQGMC::cfg_data_t
- clearCurve() : Plotter
- clearUSB() : GQLLC::GQGMC
- closeUSB() : GQLLC::GQGMC
- communicate() : GQLLC::GQGMC
- curveMap : Plotter
- curZoom : Plotter

### - d -

- dataReadAddress0 : GQLLC::GQGMC::cfg_data_t
- dataReadAddress1 : GQLLC::GQGMC::cfg_data_t
- dataReadAddress2 : GQLLC::GQGMC::cfg_data_t
- dataSaveAddress0 : GQLLC::GQGMC::cfg_data_t
- dataSaveAddress1 : GQLLC::GQGMC::cfg_data_t
- dataSaveAddress2 : GQLLC::GQGMC::cfg_data_t
- drawCurves() : Plotter
- drawGrid() : Plotter

### - e -

- eraseConfigurationData() : GQLLC::GQGMC

### - g -

- getAutoCPS() : GQLLC::GQGMC
- getBatteryVoltage() : GQLLC::GQGMC
- getConfigurationData() : GQLLC::GQGMC
- getCPM() : GQLLC::GQGMC
- getCPS() : GQLLC::GQGMC
- getDataSaveAddress() : GQLLC::GQGMC
- getErrorCode() : GQLLC::GQGMC
- getErrorText() : GQLLC::GQGMC
- getHistoryData() : GQLLC::GQGMC
- getSaveDataType() : GQLLC::GQGMC
- getSerialNumber() : GQLLC::GQGMC
- getVersion() : GQLLC::GQGMC
- GQGMC() : GQLLC::GQGMC
- graphicModeOnOff : GQLLC::GQGMC::cfg_data_t

### - h -

- HexCharStruct() : HexCharStruct

### - i -

- idleDisplayMode : GQLLC::GQGMC::cfg_data_t
- idleTitleDisplayMode : GQLLC::GQGMC::cfg_data_t
- isBigEndian() : GQLLC::GQGMC

### - k -

- keyPressEvent() : Plotter

### - l -

- loadConfigurationData() : GQLLC::GQGMC

### - m -

- Margin : Plotter
- maxBytes : GQLLC::GQGMC::cfg_data_t
- maxCPMHiByte : GQLLC::GQGMC::cfg_data_t
- maxCPMLoByte : GQLLC::GQGMC::cfg_data_t
- maxX : PlotSettings
- maxY : PlotSettings
- mBig_endian : GQLLC::GQGMC
- mCFG_Data : GQLLC::GQGMC
- mCPS_is_on : GQLLC::GQGMC
- mError_code : GQLLC::GQGMC
- mFirmware_revision : GQLLC::GQGMC
- mHistory_data : GQLLC::GQGMC
- minimumSizeHint() : Plotter
- minX : PlotSettings
- minY : PlotSettings
- mouseMoveEvent() : Plotter
- mousePressEvent() : Plotter
- mouseReleaseEvent() : Plotter
- mRead_status : GQLLC::GQGMC
- mUSB_device : GQLLC::GQGMC
- mUSB_serial : GQLLC::GQGMC
- myTimerID : Plotter

### - n -

- nCounterDelayHiByte : GQLLC::GQGMC::cfg_data_t
- nCounterDelayLoByte : GQLLC::GQGMC::cfg_data_t
- nPowerSavingMode : GQLLC::GQGMC::cfg_data_t
- nSensitivityAutoModeThreshold : GQLLC::GQGMC::cfg_data_t
- nSensitivityMode : GQLLC::GQGMC::cfg_data_t
- numXTicks : PlotSettings
- numYTicks : PlotSettings
- nVoltageOffset : GQLLC::GQGMC::cfg_data_t

### - o -

- openUSB() : GQLLC::GQGMC

### - p -

- paintEvent() : Plotter
- pixmap : Plotter
- PlotSettings() : PlotSettings
- Plotter() : Plotter
- powerOnOff : GQLLC::GQGMC::cfg_data_t

### - r -

- readCmdReturn() : GQLLC::GQGMC
- refreshPixmap() : Plotter
- resetDataSaveAddress() : GQLLC::GQGMC
- resizeEvent() : Plotter
- rubberBandIsShown : Plotter
- rubberBandRect : Plotter

### - s -

- sampleCnt : Plotter
- saveDataType : GQLLC::GQGMC::cfg_data_t
- saveDateTimeStampByte0 : GQLLC::GQGMC::cfg_data_t
- saveDateTimeStampByte1 : GQLLC::GQGMC::cfg_data_t
- saveDateTimeStampByte2 : GQLLC::GQGMC::cfg_data_t
- saveDateTimeStampByte3 : GQLLC::GQGMC::cfg_data_t
- saveDateTimeStampByte4 : GQLLC::GQGMC::cfg_data_t
- saveDateTimeStampByte5 : GQLLC::GQGMC::cfg_data_t
- scroll() : PlotSettings
- sendCmd() : GQLLC::GQGMC
- sendKey() : GQLLC::GQGMC
- setCurveData() : Plotter
- setPlotSettings() : Plotter
- setSaveDataType() : GQLLC::GQGMC
- sizeHint() : Plotter
- spanX() : PlotSettings
- spanY() : PlotSettings
- spare : GQLLC::GQGMC::cfg_data_t
- speakerOnOff : GQLLC::GQGMC::cfg_data_t
- startSample() : Plotter
- swivelDisplay : GQLLC::GQGMC::cfg_data_t

### - t -

- timerEvent() : Plotter
- turnOffCPS() : GQLLC::GQGMC
- turnOffPower() : GQLLC::GQGMC
- turnOnCPS() : GQLLC::GQGMC

### - u -

- updateConfigurationData() : GQLLC::GQGMC
- updateRubberBandRegion() : Plotter

### - w -

- wheelEvent() : Plotter
- writeConfigurationData() : GQLLC::GQGMC

### - z -

- zoomByte0 : GQLLC::GQGMC::cfg_data_t
- zoomByte1 : GQLLC::GQGMC::cfg_data_t
- zoomByte2 : GQLLC::GQGMC::cfg_data_t
- zoomByte3 : GQLLC::GQGMC::cfg_data_t
- zoomIn() : Plotter
- zoomInButton : Plotter
- zoomOut() : Plotter
- zoomOutButton : Plotter
- zoomStack : Plotter

### - ~ -

- ~GQGMC() : GQLLC::GQGMC

All Classes Namespaces Files Functions Variables Enumerations Enumerator