Data logger/monitor app for the GQ Electronics GMC-300 Geiger Counter
written by Nick Cannata njc@njctech.com in python

geiger.exe or geiger.py should be run with -c commandline argument to specify com port.  All other switches are optional (use -h or --help)


geiger.ini is required - see this file for more information
See dbCreateTable.txt to create the appropriate SQL table 

Events are logged to geiger.log
Data is logged to radiation.log (switchable and per filename defined in the INI file)



Dependencies:

If you want to make changes to the source, feel free.  You will need the following packages in addtion to python 2.7.x:

pyodbc
pyserial
colorama
pyinstaller (if you want to compile to an exe.


NOTE:	All testing and development was done on Windows x86 and x64 platforms.  Some configurations are specific to windows, 
	however there is no reason that with a little minor tweaking you can't get this running on Mac OS or a *nix kernel.